> QoS Policer Configuration
> This screen allows you to configure a QoS policer.
> Click 'Apply/Save' to save the policer.
> Notes:
> --For TwoRateThreeColor policer, Peak Rate shall be higher than Committed Rate.
> --CBS and EBS shall be minimally larger than the size of the largest possible IP packet in the stream.
> --PBS shall be minimally larger than CBS by the size of the largest possible IP packet in the stream.

> Name: |
> Enable: |
> Meter Type: |
> Committed Rate (kbps): |
> Committed Burst Size (bytes): |

> Excess Burst Size (bytes): |

> Peak Rate (kbps): |
> Peak Burst Size (bytes): |

> Conforming Action: |  |

> Partial Conforming Action: |  |

> Nonconforming Action: |  |