> QoS Queue Configuration
> This screen allows you to configure a QoS queue and add it to a selected layer2 interface.

> Name: |
> Enable: |
> Interface: |

> Queue Precedence: | (lower value, higher priority)

> - The precedence list shows the scheduler algorithm configured at each precedence level.
> - Note that precedence level with SP scheduler may have only one queue.
> - precedence level with WRR/WFQ scheduler may have multiple queues.

> Scheduler Algorithm

> Strict Priority

> Weighted Round Robin

> Weighted Fair Queuing

> Queue Weight: | [1-63]

> Drop Algorithm

> DT (Drop Tail)

> RED (Random Early Detection)
> Minimum Threshold: | [1-100]% of queue size
> Maximum Threshold: | [1-100]% of queue size

> WRED (Weighted RED)
> Low Class Min Threshold: | [1-100]% of queue size
> Low Class Max Threshold: | [1-100]% of queue size
> High Class Min Threshold: | [1-100]% of queue size
> High Class Max Threshold: | [1-100]% of queue size

> DSL Latency: |