- Quick Tasks
- Setup Port Forwarding
- Run Quick Start Wizard
- Reboot Router
- Log Out

## QoS Queue Setup

### QoS

- Basic
- Queue
- Classification
- Port Shaping

In ATM mode, a maximum of 16 queues can be configured.

In PTM mode, a maximum of 8 queues can be configured.

For each Ethernet interface, there is a maximum of 4 queues that can be configured.

For each Ethernet WAN interface, there is a maximum of 8 queues that can be configured.

Name | Key | Interface | Qid | Prec/Alg/Wght | DSL Latency | PTM Priority | Shaping Rate (bps) | Min Bit Rate (bps) | Burst Size (bytes) | Enable | Remove
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Default Queue | 65 | ptm0 | 1 | 8/WRR/1 | Path0 | Low |  |  |  | Enable | Delete
Default Queue | 66 | atm0 | 1 | 8/WRR/1 | Path0 |  |  |  |  | Enable | Delete

Add

## Add Queue

This screen allows you to configure a QoS queue and assign it to a specific layer2 interface. The scheduler algorithm is defined by the layer2 interface.

Name:
Enable
Interface
Queue Precedence:

- The precedence list shows the scheduler algorithm configured at each precedence level.
- Note that precedence level with SP scheduler may have only one queue.
- precedence level with WRR/WFQ scheduler may have multiple queues.

Scheduler Algorithm: Weighted Round Robin Weighted Round Robin Weighted Fair Queuing
Queue Weight: [1-63]
Minimum Rate: [1-965 Kbps] (-1 indicates no shaping)
Shaping Rate: [1-965 Kbps] (-1 indicates no shaping)
Shape Burst Size: [bytes] (shall be >=1600)
PTM Priority:
DSL Latency:
Close
View Wlan Queue Setup

## QoS Wlan Queue Setup

Note: If WMM function is disabled in Wireless Page, queues related to wireless will not take effects.

Name | 55Key | Interface | Qid | Prec/Alg/Wght | Enable
--- | --- | --- | --- | --- | ---
WMM Voice Priority | 1 | wl0 | 8 | 1/SP
| Enabled
WMM Voice Priority | 2 | wl0 | 7 | 2/SP
| Enabled
WMM Video Priority | 3 | wl0 | 6 | 3/SP
| Enabled
WMM Video Priority | 4 | wl0 | 5 | 4/SP
| Enabled
WMM Best Effort | 5 | wl0 | 4 | 5/SP
| Enabled
WMM Background | 6 | wl0 | 3 | 6/SP
| Enabled
WMM Background | 7 | wl0 | 2 | 7/SP
| Enabled
WMM Best Effort | 8 | wl0 | 1 | 8/SP
| Enabled
WMM Voice Priority | 33 | wl1 | 8 | 1/SP
| Enabled
WMM Voice Priority | 34 | wl1 | 7 | 2/SP
| Enabled
WMM Video Priority | 35 | wl1 | 6 | 3/SP
| Enabled
WMM Video Priority | 36 | wl1 | 5 | 4/SP
| Enabled
WMM Best Effort | 37 | wl1 | 4 | 5/SP
| Enabled
WMM Background | 38 | wl1 | 3 | 6/SP
| Enabled
WMM Background | 39 | wl1 | 2 | 7/SP
| Enabled
WMM Best Effort | 40 | wl1 | 1 | 8/SP
| Enabled

Close