- Quick Tasks
- Setup Port Forwarding
- Run Quick Start Wizard
- Reboot Router
- Log Out

## Queue Management Configuration

### QoS

- Basic
- Queue
- Classification
- Port Shaping

If Enable QoS checkbox is selected, choose a default DSCP mark to automatically mark incoming traffic without reference to a particular classifier. Click 'Apply/Save' button to save it.

Note: If Enable QoS checkbox is not selected, all QoS will be disabled for all interfaces.

Note: The default DSCP mark is used to mark all egress packets that do not match any classification rules.

Enable QoS
Select Default DSCP Mark: