> IPSec Settings

> IPSec Connection Name |
> Tunnel Mode |

> Remote IPSec Gateway Address (IP or Domain) |
> Tunnel access from local IP addresses |

> IP Address for VPN |

> Mask or Prefix Length |

> Tunnel access from remote IP addresses |

> IP Address for VPN |

> Mask or Prefix Length |

> Key Exchange Method |

> Authentication Method |

> Pre-Shared Key |

> Certificates |

> Perfect Forward Secrecy |
> Advanced IKE Settings |

> Encryption Algorithm |
> Encryption Key |
> | Hex value: DES - 16 digit, 3DES - 48, AES 32, 48, 64 digit
> Authentication Algorithm |
> Authentication Key |
> | Hex value: MD5 - 32 digit, SHA1 - 40 digit
> SPI |
> | Hex value: 100-FFFFFFFF

> Phase 1
> Mode |
> Encryption Algorithm |
> Integrity Algorithm |
> Select Diffie-Hellman Group for Key Exchange |
> Key Life Time | Seconds
> Phase 2
> Encryption Algorithm |
> Integrity Algorithm |
> Select Diffie-Hellman Group for Key Exchange |
> Key Life Time | Seconds